How to install VAG 24.7 in the PC

This cable suggests not using the internet, official software usage can often be blocked.

a. Turn off antivirus such as AVG, McAfee, etc.

b. Disable Windows Defender

c. Block vcds on the firewall (PC firewall is not turned off).

Installation Guide:

1. Install VCDS-Release-24.7.-Installer.exe Step by Step (If your system is 64-bit, you must install 32-bit to 64-bit)

2. If the installation was successful, please do not run the vcds release 24.7 software and delete the shortcuts for the computer desktop VCDS version 24.7.

3. Copy the CD program VCDSLoader.exe into the installation folder (C: Ross-Tech / VCDS) and create the shortcut to your desktop.

4.First time to plug cables into the PC, wait a while to run VCDSLoader.exe. Click Options to run the self-test, and then click Save Data.

5. Turn off all vcds software, plug in your car, and run VCDSLoader.exe again.

Note: If you need to unplug your antivirus, release 24.7 is original software, you will need to use VCDSLoader.exe to not simply block cables.